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Audi A8 Current Flow Diagram No. 12/2

Central locking, interior locking switch

u - 30 D -
< 14 E150 - Interior locking switch, driver's side
3 E S1 - Fusein fuse carrier
5 -
Ti0e - 10-pin connector, green, connector point, wheelhouse, right
T10h - 10-pin connector, red, connector point, wheelhouse, right =
T100 - 10-pin connector, connector plug B at V94
T10r - 10-pin connector, dark brown, connector point, wheelhouse,
right
T12 - 12-pin connector, connector plug A at V94
V94 - Central locking motor with control unit for interior ights switch-
off delay and ani-theft alarm system
W - Interior ight, front
) - Connection (86s), in dash panel viring haress
) - Earth connection, in interior wiring hamess, front right

- Earth connection (front passenger’s door), in interior wiring
harness

- Earth connection (driver's door/1), in interior wiring hamess

Positive (+) connection (30, central electrics). in interior wiring

harness

- Positive (+) connection (30 a), in window liftericentral locking
and door contact switch wiring hamess

- Positive (+) connection (30 a). in window lifter/central locking

and door contact switch wiring hamess
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Audi A8 Current Flow Diagram No. 12/3

Contact switch in lock cylinder for tailgate/bootlid/anti-theft alarm

systemicentral locking system, door handle switch
2 i F121 - Driver's door handle switch for anti-theft alarm
X x F122 - Front passenger's door handle switch for anti-theft alarm
“ & F124 - Contact switch in lock cylinder for tailgate/bootlid/anti-theft
{ > alarm system/central locking system
R -
IO - 104 3
Tor -
™o
T16 - 16-pin connector, connector plug C at V34
V84 - Central locking motor with control unit for interior lights switch- =
off delay and anti-theft alarm system
W3 - Luggage compartment light

- Earth connection, in tailgate/bootid wiring hamess

- Earth connection (front passenger’s door), in interior wiring
harness

- Earth connection (driver's door/1), in interior wiring hamess

W: W3

1l <

>

©D)

A4

- Connection (lock cylinder open). in window liter wiring

ior uige hamees
'Fl'm.« Connection (lock cylinder closed). in window lfter wiring
hamess

0,35 0,35
- Connection (open), in anti-theft alarm system wiring hamess

- Connection (closed), in antitheft alarm system wiring hamess
- Connection (58R), in rear wiring hamess

BBDO6)

\ 4

b a
T f -
&

Inm inzrs 168
0as a3s 0as
brige bir ira

asgs=esggazys

V(402 [Audi A8 [ABZ 1





image3.png
A Sevice Edt View Settings Wamings

%| 8| D|#[@|®| 1| <[]

e —

Page 2 Central locking, interior locking switch

swenem] o] &[] 2]

20 30
15 15
X X
Bl 3

Jzas Ve Var
e

038 05 08

briens Vou

§T100s I“unu
15
roigr
15
br

05 25 15 25

¥ Yo
o8 le B1od

o ijl w0 Bl

2 a0 a1 32 3 3 35 3 37

aggs=asggazyy

>

v
@
EN
EN

Anti-theft alarm system horn, tailgatelbootlid contact switch for anti-
theft alarm
F123 - Tailgatefbootiid contact switch for anti-theft alarm

H8 - Antitheft alarm system horn

J218 - Combi-processor in dash panel insert

J245 - Sliding sunroof adjustment control unit

S4 - Fusein fuse carrier

Ti00 - 10-pin connector, connector plug B at V94

T10r - 10-pin connector. dark brown, connector point, wheelhouse,
right

T12 - 12-pin connector, connector plug A at V94

T16 - 16-pin connector, connector plug C at V94

T26 - 26-pin connector, red. on dash panel insert

V14 - Window lifter motor, left

V15 - Window lifter motor, right

V26 - Window lifter motor, rear left

V27 - Window lifter motor, rear right

V94 - Central locking motor with control unit for interior lights switch-
off delay and anti-theft alarm system

@ - Earth point, near left tail light

%) - Earth point, near right tai light

- Earth connection, in tailgate/bootid wiring hamess
- Earth connection,

ing hamess, rear right

ing harness, rear left

@ - Connection (convenience), in window lifter wiring hamess.
@ - Connection, in central locking wiring harness.
@ - Connection(15a), i rear wiring hamess
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Anti-theft alarm system contact switch
F120 - Antitheft alarmirodent repellent system contact switch

2 » J234 - Airbag control unit
X X R47 - Centrallocking and antitheft alarm system aerial
3 T100 - in connector, connector plug B at V34
{ } T10r - 10-pin connector, dark brown, connector point, wheelhouse,
right
T12 - 12-pin connector, connector plug A at V94
T16 - 16-pin connector, connector plug C at V34
V84 - Central locking motor with control unit for interior lights switch-
off delay and anti-theft alarm system
@ - Earth point, lower part of right A-
m - Earth point, lower part of left A-pillar
@ - Earth connection, ing harness, front right
@ - Earth connection, in i jiring hamess, front left
. IS @ - Earth connection, in dash panel wiring hamess
L Ra7 @ - Connection (left tur signal). in rear wiring harness
< b @ - Connection (right turn signal), in rear wiring harness
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Door contact switch
F2 - Door contact switch, driver's side
2 n F10 - Rearleft door contact switch
% X F11 - Rear right door contact switch
U136 - Seat adjustment with memory control unit
4218 - Combi-processor in dash panel insert
Téb - 6-pin connector, grey, connector point, wheslhouse, right
T16 - 16-pin connector, connector plug C at V34
T26a - 26-pin connector, green, on dash panel insert

T26b - 26-pin connector, yellow, on dash panel insert

V84 - Central locking motor with control unit for interior lights switch-
off delay and anti-theft alarm system
W9 - Leftfootwelllight

W31 - Frontleft entry light
W33 - Rear left entry light
W34 - Rear right entry light
- Earth connection, in interior wiring hamess, front left

(
A @ - Earth connection (rear right), in interior wiring harness
W g € ® (s - Earth connection (criver's door/1), i interior wiring harmess
035 035 - Connection (door contact switch, left), in window lifter/central
uign e locking and door contact switch viring hamess
' @ - Connection (door contact switch, right and left), in
2 ,riosdriond rrans Ifterlcentrallocking system and door contact s

hamess
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Interior monitor, ultra-sonic sensors control uni

1 b4 E18 - Rear fog light switch
X X E183 - Interior monitor switch
3 n F3 - Frontright door contact switch
G170 - Leftultra-sonic sensor for anti-theft alarm system
G171 - Right ultra-sonic sensor for antitheft alarm system
4218 - Combi-processor in dash panel insert
4347 - Ultra-sonic sensors control unit
K95 - Alarm system warning lamp
T10r - 10-pin connector, dark brown, connector point, wheelhouse,
right
T26 - 26-pin connector, red, on dash panelinsert
G V2 - Fresh air blower

‘ W10 - Right footwell light
3 W32 - Frontright entry light

i I I‘= () - Esrth poin, lower part of right A-pilar

A - Earth connection (front passenger’s door), in interior wiring

harness
- Earth connection (rear right)

terior wiring hamess
- Earth connection, in interior wiring hamess, rear left

(o)
(&)
- Connection (door contact switch, right), in window lifter/central

locking and door contact switch

- Connection (door contact switch, right and left), in window

lifter/central locking system and door contact switch wiring
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