	[bookmark: _GoBack]Removing and installing steel wheel bearing housing
Servicing wheel bearing housing with pressed-in wheel bearing
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	1. [bookmark: QWPdtPROG]Wheel bearing housing
For wheel bearing with outer-ø 85 mm, or 82 mm, respectively.
It is permissible to install e.g. ø 85 on left and ø82 on right side.
· ◆ Removing and installing
=>Page 40-30
1. Wheel bearing
0. ◆ Always replace
0. ◆ Installation position:
0. ‒ Large internal diameter of wheel bearing faces wheel hub
0. ◆ Pressing out =>Fig. 2
0. ◆ Pulling off bearing inner race => Fig.3
0. ◆ Pressing in => Fig. 4
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	1. Wheel hub
0. ◆ Stepped version
0. ◆ Pressing out =>Fig. 1
0. ◆ Pressing in => Fig. 5
1. Hexagon bolt, 10 Nm
1. Cover plate
1. Speed sensor
3. ◆ Pull out to remove
3. ◆ Before inserting sensor, clean fitting hole inner surface and coat with lubricating paste G 000 650.
3. ◆ Routing => Page 40-21
1. Sleeve
4. ◆ Grease all around with lubricating paste G 000 650 before inserting in wheel bearing housing
4. ◆ Press up to stop into wheel bearing housing
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	→ Fig.1    Pressing out wheel hub
	[bookmark: 6Wvmd136BAIE]
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	→ Fig.2    Pressing wheel bearing out of wheel bearing housing
	[bookmark: $Yvmd78BAIE]
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	→ Fig.3    Pulling bearing inner race off wheel hub
[bookmark: 9Xvmd190BAIE]Always use puller with clamp, e.g. Kukko 204- 1 (commercially available).
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	→ Fig.4    Pressing wheel bearing into wheel bearing housing
[bookmark: UYvmd3a2BAIE]For wheel bearing with outer-ø 82 mm use the thrust pad -3124-, for outer-ø 85 mm use thrust pad -3062-.
Note:
Large internal diameter of wheel bearing faces wheel hub
· ‒ Press wheel bearing -A- in up to stop.
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	→ Fig.5    Pressing wheel hub into wheel bearing
· [bookmark: jWvmdf0BAIE]‒ When pressing in, thrust pad -VW 447i- must only make contact with the bearing inner race.
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