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C - Altemator

D - Ignition/starter switch

E1 - Lighting switch

E4 - Headight dipperfiasher switch

J59 - X contact relief relay

JS0 - Daytime driving light switch-on relay

J218 - Combi-processor in dash panel insert

K& - Side light warning lamp

S5 - Fuseinfuse carrier

TH0i - 10-pin connector, yellow, in centre console
T14 - 14-pin connector, purple, behind steering column switch trim

T26b - 26-pin connector, yellow, on dash panel insert
- Positive (+) connection (15), in dash panel wiring hamess

- Connection (1), in dash panel wiring hamess
- Connection (75s). in dash panel wiring hamess
- Positive (+) connection (30), in dash panel wiring hamess

- Earth connection, in dash panel wiring hamess (near relay point)
- Connection (left-hand parking light). in dash panel wiring haness
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(‘; - Positive (+) connection (30). in Motronic wiring hamess
(=)
(=
(=%

- Connection (right-hand parking light),in dash panel wiring hamess
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Current Flow Diagram

No. 24/3
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Daytime driving lights with fog lights.

E102 - Headight range control adjuster
2 n J123 - Bulb monitoring device
% X K1 - Main beam waming lamp

122 - Foglight bulb, left

123 - Foglight bulb, right

M1 - Sidelight bub, left

M3 - Sidelight bulb, right

M29 - Dipped beam bulb, left
M30 - Main beam bulb, left
M31 - Dipped beam bulb, right
M32 - Main beam bulb, right

$1 - Fuseinfuse carrier
S2 - Fuseinfuse carrier
$3 - Fuseinfuse carrier
S4 - Fuseinfuse carrier
S5 - Fuseinfuse carrier
A S5 - Fuseinfuse carrier
i Q> TEh - 5-pin connector, black, on headiight, left
o | TS - 5-pin connector, black, on headight,right
~ AL 158 - 184 1 104" 104 ¥ T26a - 26-pin connector, green, on dash panel insert
i *we I 1° V48 - Headlight range control motor, left
0 e V49 - Headlight range control motor. right
05 45 45 40 48 48 45 SN (=) - Earth connection -1~ infront let wiring hamess
€1 omse  Caavme oolbr geion oen web whge waige e o e
N (e @, - arth connection -1-,in front right wiring hamess
as 10 15 0,38 %) - Connection (56), in dash panel wiring haress
srios acian  gein weige waige SN

@ - Positive (+) connection (58L), in front left wiring harness.
@ - Positive (+) connection (58R), in front left wiring hamess

rvR K1
[J1zs | @ - Connection (56b) -1-, in front lighting wiring hamess
I‘““"‘"‘ =) - Connection (56a, right). in dash panel wiring hamess |
@ @ 4
9
a5 h0 0 os s s Ve
oige g  an arws geiaw
53LI 1 I e .
385 Yrsma Frsin e Besis Besus rswa Brsia
M1 & L2270 Las M3 Msi Mas < Mao.
et
25 28
b br
l=]
5 8 7 B 19 o, m m m oz s W m
VT Overin ) Current flow diagram
Foroso 0000076885 | v (452 [Audi A8 [ACK | I I [l
e servi 246
suncn| | [) tectromc serve . K




image3.png
[Current flow diagras
A service Edt View Settings Warmings 7

MEIE
=181

8| &) Dlofale| w1 il « 0| 3| =I| Blolgle|s/s Slolelalalglzls] | woal &

Page 3: Daytime drivng ights with fog ihts

e — I

R e e BN B

Audi A8

Current Flow Diagram

No. 24/4

30

18

El

s‘rz[} >
Esr
e K
o oET b
,,, n orign
P V7 V7 /
25 25 10 a5 o 1o o5 A a5 o
brige golmw walbl arige oriws otgn srgn ion aeign
Kool wm JTm./v 23

,.;m Tiaar
T st

10
25 ] 25 n.; 05 arign
% wmw ﬂmu 1

2 05

i-rm]nm T" ws

10 10 05 05 a5
ariaw  griro

&

-
S
-

—

e

Ma Mz

Mz
' |
1

E
%
x
x

I
|
.!
|

2 3 3 32 3.3 3 35 37 3 3 a0 a

s
£

aggs=aEggaagy

>

v
@
EN
EN

Daytime driving lights with fog lights
E87 - Control and display unit for air conditioner
J5 - Foglight relay

J89 - Daytime driving light change-over relay
4123 - Bulb monitoring device

M2 - Taillight bulb, right

M4 - Taillight bulb, left

N74 - Resistance wire

$3 - Fuseinfuse carrier

- 2-pin connector, brown, electronics box, front passenger's footwell
- 6-pin connector, white, connector point, wheelhouse, right

- 10-pin connector, green, connector point, wheelhouse, right

- 10-pin connector, yellow, in centre console

- Number plate light

- Earth connection, in tailgate/bootid wiring hamess

- Connection (58a), in dash panel wiring hamess.

- Connection (fog light),in front lighting wiring hamess

- Earth connection, in dash panel wiring hamess (near relay point)

- Positive (+) connection (58), in rear wiring hamess
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Audi A8 Current Flow Diagram No. 24/5

Daytime driving lights with fog lights

3 * P2 E7 - Fog light switch
X X E18 - Rear fog light switch
3 31 J218 - Combi-processor in dash panel insert
J347 - Uttra-sonic sensors control unit
K35 - Alarm system wamning lamp
L40 - Frontand rear fog light switch illumination bulb
L46 - Rearfog light bulb, left
S1 - Fusein fuse carrier
Téb - 6-pin connector, grey, connector point, wheslhouse, right
T6f - 6-pin connector, black, on dash panel insert
T10r - 10-pin connector, dark brown, connector point, wheslhouse, right

@ - Earth connection, in tailgate/bootlid wiring harness
(;1}, - Connection (58d), in dash panel wiring hamess.

m - Positive (+) connection (30, central electrics),
- Earth connection (centre console), in dash panel wiring hamess
Positive (+) connection (30 a), in window lfter/central locking and door contact switch wiring hamess

interior wiring hamess

b4
BBD)

Connection (rear fog light), in rear wiring hamess
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