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Audi A8 Current Flow Diagram No. 61/1°

Edition 07.1995

Radio gamma, delta sound system, radio-Bose sound system with and without CD changer
Model year 1996
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1- Fuse carrier 1 (ST1), black
2- Fuse carrier 1 (ST2), red
3- Fuse carrier 1 (ST3), yellow
4- Fuse carrier 1(ST4), blue
5- Fuse carrier 1 (ST5), brown
8- Radiator fan fuse (S42)
7 - Spare fuses

A, B, C. Screwed junctions
b7

Relay and fuse carrier, luggage compartment, right

Position of relays
1- Terminal 30 junction box
7 - Radio fuse (S92)
Fuse colours:
30A- green
25A- white
20A- yellow
15 A~ blue
10A- red
5A- beige
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Radio gamma, delta sound system, radio-Bose sound system with and without CD changer
A - Battery

4218 - Combi-processor in dash panel insert
J383 - Audio steering wheel printed circuit board

R - Radio

S92 - Radio fuse

Ttk - Single connector, brown, in centre console

Tsb - 5-pin connector, black. behind steering column switch trim

T6c - 6-pin connector, dark brown, connector point, wheelhouse, right

Téh - 6-pin connector, green, radio connector 1-2
T8 - 8-pin connector, black, radio connector i

Ti0i - 10-pin connector, yellow, i centre console

T16 - 16-pin connector, connector plug C at Va4

T26 - 26-pin connector, red, on dash panel insert

TV2 - Terminal 30 junction box

V84 - Centrallocking motor with control unit for interior lights switch-off delay and anti-theft alarm system
@ - Earth point, lower part of right A-pillar

@ - Earth connection, in radio wiring hamess.

@ - Connection (speed signal), in dash panel wiring hamess

m - Positive (+) connection (30), in rear loudspeaker wiring hamess

- Radio gamma, delta sound system
- Radio-Bose-sound system
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Audi A8

Current Flow Diagram No. 61/3
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Radio gamma, delta sound system, radio-Bose sound system with and without CD changer
R - Radio

R14 - Treble loudspeaker, rear left

R15 - Bass loudspeaker, rear left

R16 - Treble loudspeaker, rear right

R17 - Bass loudspeaker, rear right

R21 - Bass loudspeaker, front left

R23 - Bass loudspeaker, front right

R26 - Middle-high tone loudspeaker, front left
R27 - Middle-high tone loudspeaker, front right
R34 - Middle-treble tone loudspeaker, rear left
R35 - Middle-treble tone loudspeaker, rear right

T5d - 5-pin connector, on loudspeaker rear left, under rear shelf
Tse - 5-pin connector, on loudspeaker rear right, under rear shelf
T6g - 6-pin connector, yellow, radio connector I

T8b - 8-pin connector, brown, radio connector II

@ - Earth connection, in loudspeaker wiring hamess
@ - Connection (negative, loudspeaker) in loudspeaker wiring hamess
- - Radio gamma, delta sound system
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Current flow.

Audi A8 Current Flow Diagram No. 61/4

Radio gamma, delta sound system, radio-Bose sound system with and without CD changer

J371 - Telephone isolation relay
b b R - Radio
X X R12 - Amplifier
Ri5 - Bass loudspeaker, rear left
RI7 - Bass loudspeaker, rear right
R20 - Treble loudspeaker, front left
R21 - Bass loudspeaker, front left
R22 - Treble loudspeaker, front right
R23 - Bass loudspeaker, front right
R34 - Middle-treble tone loudspeaker, rear eft
@ N R35 - Middle-treble tone loudspeaker, rear right
SR NS Rt R3 - Telephone transmitter and receiver unit
¥ o § ¢ R41 - CD changer
J Tég - 6-pin connector, yellow, radio connector I-1
b i T8a - 8-pin connector, blue, radio connector I3
: - @ - Earth connection, in loudspeaker wiring hamess
osr st o5 ogr asr osr s - Only models with CD changer
o guws o b ge rows < > - - Radio-Bose-sound system

Models without telephone
- Models with telephone, near frequency divider i rear left luggage compartment
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Current Flow Diagram No. 61/5

Audi A8
Radio gamma, delta sound system, radio-Bose sound system with and without CD changer
30 30 A - Battery
' 2 D - Ignition/starter switch
El 3 4218 - Combi-processor in dash panel insert
R - Rado
R36 - Telephone transmitter and receiver unit
Tz - 3-pin connector, black, near aerial motor
T6f - 6-pin connector, black, on dash panel insert
T8 - 8-pin connector, black, radio connector Il
Ti0e - 10-pin connector, green, connector point, wheelhouse, right
A Ti0i - 10-pin connector, yellow, in centre console
T12 - 12-pin connector, connector plug A at Va4
1 Rz | T26b - 26-pin connector, yellow, on dash panel insert
1Z0 60 R_7 28 V21 - Aerial motor
T 5 'I“ - Central locking motor with control unit for interior lights switch-off delay and anti-theft alarm system
J—L/ = 30 m - Earth point, near right tail light
(=1 ; A - Earth connection, in loudspeaker wiring harness
ka1 Ao - Connection (58), in dash panel wiring hamess
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- Positive (+) connection (30), in dash panel wiring hamess
- Positive (+) connection (30), in Motronic wiring hamess
Models with telephone

Va4
)

()

% - Connection (86s). in dash panel wiring hamess
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