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Page 3: Starter inhbtor relay, automatic gearbox control urit

"Automatic gearbox control unit, Tiptronic switch, selector lever lock solenoid
" w F189 - Tiptronic switch
i 8 4217 - Automatic gearbox control unit
X % J218 - Combi-processor in dash panel insert
L19 - Gear selector light bulb
L79 - Selector lever ilumination
L9 - +- Display illumination (automatic gearbox)
N110 - Selector lever lock solenoid
T2ae - 2-pin connector, black, in selector lever console
Joe du T2af - 2-pin connector, yellow, in selector lever console
itz T5f - 5-pin connector, red. in selector lever console
T Tog - 5-pin connector, black, in selector lever console
TI0 - 10-pin connector, blue, connector point, electronics box, plenum chamber
oow T10b - 10-pin connector, yellow, connector point, electronics box, plenum chamber
Toos W Tio0 W Tioos Ti0c - 10-pin connector, green, connector poit, electronics box, plenum chamber
7 Ti0g - 10-pin connector, black, near selector lever console.
T32%b - 32-pin connector, grey, on dash panel insert
s s Gk ae o ox o= A (i) - Earthconnecton, in gearbox wiing hamess
< > () - Posilive (+) connection (58d), in dash panel wiring hamess (display illumination)
ng ‘rmn ng Tooa Tﬁm Trogz. oS @ - Earth connection (centre console), in dash panel wiring haress
* - Models with Tiptronic
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Audi A8 Current Flow Diagram No. 8/7
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Audi A8 Current Flow Diagram No. 8/7 i

Brake light switch, cruise control system brake pedal switch (diesel direct injection system)

0 " D - lgnitionistarter switch
i *: i E1 - Lighting switch
£ H] F - Brake light switch

J104 - ABS with EDL control unit
J123 - Bulb monitoring device, front
4220 - Motronic control unit

‘ F47 - Cruise control system brake pedal switch (diesel direct injection system)

J248 - Diesel direct injection system control unit

M9 - Brake light bulb, left

M10 - Brake light bulb, right

S3 - Fuseinfuse carrier

S9 - Fuseinfuse carrier

S10 - Fusein fuse carrier

T10b - 10-pin connector, yellow, connector point, electronics box, plenum chamber

T T14 - 14-pin connector, purple, behind steering column switch trim

- Positive (+) connection (15). in dash panel wiring hamess

>

- Connection (54), in dash panel wiring hamess
- Connection (58a), in dash panel wiring hamess.

(=)

ar
(m} - Positive (+) connection -4- (15a), in interior wiring hamess
(=»

- Connection (872), in engine wiring harness

ST2.

Connection (30, central electrics), in dash panel wiring hamess

Models with petrol engines
Models with diesel engines
Only models with ABS and ESP
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Page 3: Starter inhbtor relay, automatic gearbox control urit

Audi A8 Current Flow Diagram No. 8/1

Automatic gearbox (01V) with 8-cylinder engines, 3.7 litre, 191 kW, AKC and 6-cylinder engines, 2.8
litre, 142 kW, AMX and 2.5 litre, 110 kW (TDI), AKE
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Page 3: Starter inhbtor relay, automatic gearbox control urit

Audi A8 Current Flow Diagram No. 8/2
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8 -5 montorng dnics 4125
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Positon of relays:
Y - Automatc gearbconrl uifuse (pol angins) (5113)

- Autmatcgaabox conol unt s (esel engines) (5113)
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Page 3: Starter inhbtor relay, automatic gearbox control urit

S204 - Fuse-1-(30)
T2ad - 2-pin connector, black, near altemator, in engine compartment, front right

TI0 - 10-pin connector, blue, connector point, electronics box, plenum chamber
Ti0a - 10-pin connector, black, connector point. electronics box, plenum chamber
TH0c - 10-pin connector, green, connector point, electronics box. plenum chamber

T10d - 10-pin connector, red, connector point. electronics box, plenum chamber
- Connection (30c). in dash panel wiring hamess

- Connection (502), in dash panel wiring hamess.
Connection (multi-function switch), in dash panel wiring hamess

>

Connection (30, central electrics), in dash panel wiring hamess

Positive (+) connection (30), in diesel direct injection system wiring harness

Models with petrol engines
Models with diesel engines

PDODD);

v
@
EN
EN

AUUr AS CUITENT T 1O Dragramt NO. 07 Z

Starter inhibitor relay, automatic gearbox control unit

» o - @ A - ety

8 i B - Starter

1S 5 D - Ignition/starter switch
J207 - Starter inhibitor relay
J217 - Automatic gearbox control unit
4220 - Motronic control unit
S113 - Automatic gearbox control unit control unit
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Audi A8 Current Flow Diagram No. 8/3 —

ic gearbox control unit, multi-fun

w " D - Ignitonistarter switch
i i F125 - Multi-function switch
H 5 J217 - Automatic gearbox control unit
K - Diagnosis connection
M16 - Reversing light bulb, left
M17 - Reversing light bulb, right
$6 - Fusein fuse carier
Tée - 6-pin connector, brown, connector point, electronics box, plenum chamber
TI0 - 10-pin connector, blue, connector point, electronics box, plenum chamber
Ti0a - 10-pin connector, black, connector point, electronics box, plenum chamber
TH0m - 10-pin connector, grey, footwell,right, at wheelhouse, behind carpet
05 o5 T10ab - 10-pin connector, black, on gearbox
gniro oo T16a - 16-pin connector, diagnosis connection
Toos !mm @ Earth connection, in gearbox wiring hamess.
K @ - Positive (+) connection (15), in dash panel wiring hamess
o A - Connection (15a, fuse 6), in dash panel wiring hamess
E

2

] > @ - Connection (diagnosis wire K), in dash panel wiring harness

L Jat7 @ - Connection (RL), in dash panel wiring harness
2

- Connection -1- (15), in automatic gearbox wiring harness
rs " rr r
+ L

os* o0s%** 05 o5 os o5

5
n ol oo s onige

- Models with petrol engines
- Models with diesel engines L

| Tioatffl Tioatfg Troa Troat
L N I

Tioabrio  Thoabit ws = white:
w = bisck

0 ©

a "

b

El

b

o

W

0 i

brge o

w % v w8 o a2 =@ u s x =z

Forono 5000143955 | 1 [402 [Audis [akc [ros [ | I [l

ol — |ofotom




image5.png
[Current
A Serviee Edt Vew Settngs Wamings 7 ETEY

2| 8| Dle(a|5| 1| «|» 1] +| o] 2| =|| Ble|s|e|EfA @|e|e|a|o|@@|S] | =l
e — e — L

Audi A8 Current Flow Diagram No. 8/4

"Automatic gearbox control unit, solenoid valves, kick-down switch
" . F8 - Kickdown switch
8 ] G93 - Gearbox oil temperature sender
5 k) J217 - Automatic gearbox control unit

N8 - Solenoid valve 1

N89 - Solenoid valve 2

N9D - Solenoid valve 3

N9t - Solenoid valve 4

N92 - Solenoid valve 5
N93 - Solenoid valve §

NS4 - Solenoid valve 7

Ti0a - 10-pin connector, black, connector point, electronics box, plenum chamber
T10b - 10-pin connector, yellow, connector point, electronics box, plenum chamber
T16b - 16-pin connector, black, on gearbox

- Earth connection, in gearbox wiring hamess

- Earth connection, in dash panel wiring hamess, left

T} - Earth connection, in dash panel wiring hamess, right
< > ) - Earth connection (centre console), in dash panel wiring harness
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Page 3: Starter inhbtor relay, automatic gearbox control urit

e e— [
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Audi A8 Current Flow Diagram No. 8/5
"Automatic gearbox control unit, gearbox speed sender, gearbox input speed sender
" “ G182 - Gearbox input speed sender
i kg G195 - Gearbox output speed sender
% X J217 - Automatic gearbox control unit
4220 - Motronic control unit
4248 - Diesel direct injection system control unit
T10d - 10-pin connector, red, connector point, electronics box, plenum chamber
Ti6b - 16-pin connector, black, on gearbox
@ - Earth point, lower part of right A-pillar
® J“ @ - Connection (high bus), in dash panel wiring hamess
s o ) - Connection (low bus), in dash panel wiring haress
o g (2% - Comecton (high bus). i engine compariment wiring harness

(;}, - Connection (low bus), in engine compartment wiring hamess
@ @ T} - Earth connection, in dash panel wiring harness, right
CAN bus (data wire)

0% 0%
obr  orisw A - - Models with petrol engines.
< > = - Models with diesel engines
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