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Earth connection, in gearbox wiring hamess
Positive (+) connection (58d), in dash panel wiring hamess (display ilumination)
Earth connection (centre console), in dash panel wiring hamess

Models with Tiptronic

Audi A8 Current Flow Diagram No. 72/6
‘gearbox control unit, Tiptronic switch, selector lever lock solenoid
" w F189 - Tiptronic switch
i i 4217 - Automatic gearbox control unit
X % J218 - Combi-processor in dash panel insert
L19 - Gear selector light bulb
L79 - Selector lever ilumination
L9 - +- Display illumination (automatic gearbox)
N110 - Selector lever lock solenoid
T2ae - 2-pin connector, black, in selector lever console
Joe du T2af - 2-pin connector, yellow, in selector lever console
itz T5f - 5-pin connector, red. in selector lever console
Il25 I'ﬂ TBq - 5-pin connector, black, in selector lever console
TI0 - 10-pin connector, blue, connector point, electronics box, plenum chamber
o T10b - 10-pin connector, yellow, connector point, electronics box, plenum chamber
Tros Tis T Ti0c - 10-pin connector, green, connector poit, electronics box, plenum chamber
® Ti0g - 10-pin connector, black, near selector lever console.
T32%b - 32-pin connector, grey, on dash panel insert
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Audi A8

Current Flow Diagram

No. 72/7
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Brake light switch, cruise control system brake pedal switch (diesel direct injection system)

D
E1

F
Fa7
J104
J123
4248
Mg

Ignition/starter switch
Lighting switch

Brake light switch

Cruise control system brake pedal switch (diesel direct injection system)
ABS with EDL control unit

Bulb monitoring device, front

Diesel direct injection system control unit

Brake light bulb, left

Brake light bulb, right

Fuse in fuse carrier

Fuse in fuse carrier

Fuse in fuse carrier

10-pin connector, yellow, connector point, electronics box, plenum chamber
14-pin connector, purple, behind steering column switch trim

Positive (+) connection (15), in dash panel wiring hamess

Connection (54),in dash panel wiring hamess

Connection (58a), in dash panel wiring hamess

Positive (+) connection -4- (15a), in interior wiring hamess

Connection (87a), in engine wiring hamess

Connection (30, central electrics), in dash panel wiring hamess

Models with petrol engines

Models with diesel engines

Only models with ABS and ESP
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Audi A8 Current Flow Diagram No. 72/1

Automatic gearbox (01V) 8 cylinder engines 3.7 1, 191 kW, AQG and 6 cylinder engines 2.81, 142 kW,
APR, AQD and 2.51, 110 kW (TDI) AFB, AKN
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Audi A8 Current Flow Diagram No. 72/2
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Starter inhibitor relay, automatic gearbox control unit

A -
B R

o

PDODD);

Battery
Starter

Ignition/starter switch

Starter inhibitor relay

Automatic gearbox control unit

Motronic control unit

Automatic gearbox control unit

Fuse -1- (30)

2-pin connector, black. near altemator. in engine compartment, front right
10-pin connector, blue, connector point, electronics box, plenum chamber
10-pin connector, black, connector point, electronics box, plenum chamber
10-pin connector, green, connector point, electronics box, plenum chamber
10-pin connector, red, connector point, electronics box, plenum chamber
Connection (30c), in dash panel wiring hamess

Connection (50a), in dash panel wiring hamess
Connection (multi-function switch), in dash panel wiring hamess
Connection (30, central electrics), in dash panel wiring hamess
Positive (+) connection (30),in diesel direct injection system wiring harness

Models with petrol engines
Models with diesel engines

Current Flow Diagram
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Current Flow Diagram

No. 72/3
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‘Automatic gearbox control unit, multi-function switch
D - Ignitonistarter switch
F125 - Multifunction switch
J217 - Automatic gearbox control unit
K - Diagnosis connection
M16 - Reversing light bulb, left
M17 - Reversing light bulb, right
$6 - Fusein fuse carier
Tée - 6-pin connector, brown, connector point, electronics box, plenum chamber
T8l - 8-pin connector, black, on gearbox
T10 - 10-pin connector, blue, connector point, electronics box, plenum chamber
Ti0a - 10-pin connector, black, connector point, electronics box, plenum chamber
TH0m - 10-pin connector, grey, footwell,right, at wheelhouse, behind carpet
Ti6a - 16-pin connector, diagnosis connection
@ - Earth connection, in gearbox wiring hamess.

2 - Positive (+) connection (15). in dash panel wiring hamess
- Connection (15a, fuse 6), in dash panel wiring hamess

- Connection (diagnosis wire K), in dash panel wiring hamess

2
(=)
() - Connection (RF (reversing ight),in dash panel wiring haress

Models with petrol engines
- Models with diesel engines
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[Audi A8

‘Current Flow Diagram

S

"Automatic gearbox control unit, solenoid valves, kick-down switch
F8 - Kick-down switch

i ] G93 - Gearbox oil temperature sender
5 5 J217 - Automatic gearbox control unit
N8 - Solenoid valve 1
N89 - Solenoid valve 2
N9D - Solenoid valve 3
N215 - Automatic gearbox pressure control valve -1-
N216 - Automatic gearbox pressure control valve -
N217 - Automatic gearbox pressure control valve -3
N218 - Automatic gearbox pressure control valve -4-
Ti0a - 10-pin connector, black, connector point, electronics box, plenum chamber
Ti0b - 10-pin connector, yellow, connector point, electronics box, plenum chamber
Ti6b - 16-pin connector, black, on gearbox
@ - Earth connection, in gearbox wiring hamess.
@ - Earth connection, in dash panel wiring hamess, left
A @ - Earth connection, in dash panel wiring hamess, right
] > @ - Earth connection (centre console), in dash panel wiring haress
{ Sor ' © - Does not apply to diesel engines
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[Audi A8

‘Current Flow Diagram No. 7275

2

3

® o

"Automatic gearbox control unit, gearbox speed sender, gearbox input speed sender
G38 - Gearbox speed sender

G182 - Gearbox input speed sender

4217 - Automatic gearbox control unit

4220 - Motronic control unit

4248 - Diesel direct injection system control unit

- 6-pin connector, brown, connector point, electronics box, plenum chamber

- 10-pin connector, red, connector point, electronics box, plenum chamber

- 16-pin connector, black, on gearbox

Earth point, lower part of right A-pillar

BRRDELL

T - Positive (+) connection (high bus), in engine compartment wiring hamess
LI L - Positive (+) connection (low bus), in engine compartment wiring hamess
bom e - Connection (data bus, screening), in engine compartment wiring hamess
- T} - Earth connection, in dash panel wiring harness, right
_ - - CAN bus (data wire)
o, Io, A - - Models with petrol engines
L B = - Models with diesel engines
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