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“Anti-locking brake system

A - Battery

G44 - Rearright speed sensor

G45 - Frontright speed sensor

G46 - Rearleft speed sensor

G47 - Frontleft speed sensor

J104 - ABS with EDL control unit

J105 - ABS return flow pump relay

J106 - Relay for ABS solenoid valves

J220 - Motronic control unit

J401 - Navigation system with CD drive control unit
$123 - ABS control unit fuse 1

T4l - d-pin connector, black, in centre console

T10c - 10-pin connector, green, connector point, electronics box, plenum chamber

@ - Positive (+) connection (30 - for ABS), in engine compartment wiring hamess.

@ - Connection (Hall sender signal), in engine compartment wiring hamess.

@ - Positive (+) connection (30), in Motronic wiring hamess.

* - Models with front-wheel drive

= - Models with four-wheel drive

=% - Models with navigation system

# - Models with 6-cylinder-petrol engines (from centre May 1997)
# - Models with -cylinder-petrol engines (from centre May 1997)
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“Anti-locking brake system
J104 - ABS with EDL control unit
32 32 K - Dash panel insert
X % N99 - ABS inlet valve, front right
N100 - ABS outlet valve, front right
N101 - ABS inlet valve, front left
N102 - ABS outlet valve, front left
N133 - ABS inlet valve, rear right
N134 - ABS inlet valve, rear left
N135 - ABS outlet valve, rear right
N136 - ABS outlet valve, rear left
K N166 - EDL change-over valve, front right
CTroar N167 - EDL outlet valve, front right
N168 - EDL change-over valve, front left
= N169 - EDL outlet valve, front left
9% A Ti6a - 16-pin connector, diagnosis connection
- IS m - Earth point, lower part of left A-pillar
035 @ - Connection (diagnosis wire K), in dash panel wiring harness
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Audi A8 Current Flow Diagram No. 8/4
‘Anti-locking brake system
J104 - ABS with EDL control unit
32 & 2 J248 - Diesel direct injection system control unit
X X K47 - ABS warning lamp
K86 - Traction control system waming lamp.
S1 - Fusein fuse carier
T6f - 6-pin connector, black, on dash panel insert
T26 - 26-pin connector, red, on dash panel insert
T26a - 26-pin connector, green, on dash panel insert
o @ - Positive (+) connection -1- (15), in engine compartment wiring harness
I - @ - Connection (15), in dash panel wiring hamess, right
T A L
28 Koo Kar - - Models with traction control system
T, grove g gresams a3 = - Models with V6 engine TDI 25 |
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Traction control system switch
Brake light switch

ABS with EDL control unit

Combi-processor in dash panel insert

Diesel direct injection system control unit
Fuse in fuse carrier

Fuse in fuse carrier

Fuse in fuse carrier

6-pin connector, black. on dash panel insert
Connection (54),in dash panel wiring hamess

Connection (58d), in dash panel wiring hamess
Positive (+) connection (15a), in dash panel wiring hamess
Connection (87a), in engine wiring hamess

Earth connection (centre console), in dash panel wiring hamess

Models with traction control system
Models with 6-cylinder TDI engine, 2.5 1, 110 kW, engine code AFB
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