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Page 3: A conditoner
‘Air conditioner
E87 - Control and display unit for air conditioner
b n G89 - Fresh air intake duct temperature sensor
X x G137 - Control motor potentiometer, right central vent
G139 - Control motor potentiometer, left footwell flap

G141 - Control motor potentiometer, rear footwell vent
G150 - Left vent temperature sender
G151 - Right vent temperature sender
V108 - Footwell flap control motor, left
188 V109 - Footwell flap control motor, right

{ } G140 - Right footwell fiap control motor potentiometer

n!s I V111 - Centre vent control motor, right
rel V112 - Rear footwell vent control motor
& Lo (72 - Earth connection -3-, in air conditioner wiring hamess
1 1 1 @ - Connection (5V), in air conditioner wiring hamess.
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ioner
Control and display unit for air conditioner

Control motor potentiometer, temperature flap
Control motor potentiometer, air flow flap

Control motor potentiometer, defroster flap

Control motor potentiometer, left central vent

Control motor potentiometer, central vent

Control motor potentiometer, ai recirculation fiap
Temperature flap control motor

Air flow flap control motor

Centre vents control motor

Defroster fiap control motor

Centre vent control motor, left

Air recirculation flap control motor

Earth connection -3-, in air conditioner wiring hamess

- Connection (5V), in air conditioner wiring hamess
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ioner
E1 - Lighting switch
3 b J218 - Combi-processor in dash panel insert
X X L67 - Dash panel left vent ilumination
L69 - Dash panel right vent lumination
L87 - Central rear vent lumination
L83 - Rearleftventilumination
L89 - Rearright vent ilumination
$3 - Fuseinfuse carrier
T6f - 6-pin connector, black, on dash panel insert
58a T10f - 10-pin connector, purple, connector point, wheelhouse, right
E1 T14 - 14-pin connector, purple, behind steering column switch trim
g m - Earth connection -1-, in dash panel wiring hamess
o5 1,0 1.0 @ - Positive (+) connection (58 D1), in dash panel wiring hamess
o "6":" " ! ") - Connection (584), in dash panel wiring haress
ey A () - Connection (58),in dash panel wiring hamess
Jorg ) (&) - Erthconnection, in dash panel wiring hamess
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15

ioner, engine cooling petrol engines
F18 - Radiator fan thermo-switch
3 F54 - Radiator fan thermo-switch

Bl

- Radiator fan relay
- Radiator fan 2nd speed relay
- Radiator fan 3rd speed relay
- Combi-processor in dash panel insert

B

- Fuse in fuse carrier
- Radiator fan single fuse

- 2-pin connector, brown, on radiator fan
- 26-pin connector, yellow, on dash panel insert

VI - Raditor fan

@ - Earth point, lower part of right A-pillar

m - Earth point, lower part of left A-pillar
(=) - Earth connection -

426
J101

J135

218

N39 - Radiator fan series resistor
S4

s42

T2x

T26b

. in front right wiring hamess

A (i) - Earth connection, in dual ton hor wiing hamess
< > @ - Connection (75a), in dash panel wiring hamess.
oS (E«} - Connection (30, radiator fan), in dash panel wiring hamess
- - Near ABS control unit
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ioner, engine cooling diesel engines
Radiator fan thermo-switch

Radiator fan thermo-switch

Radiator fan relay

Radiator fan 3rd speed relay

Radiator fan run-on control unit

Combi-processor in dash panel insert

Diesel direct injection system control unit

Radiator fan series resistor

Fuse in fuse carrier

Radiator fan single fuse

2-pin connector, brown, on radiator fan

10-pin connector, green, connector point, electronics box, plenum chamber
26-pin connector, yellow, on dash panel insert

Radiator fan

Earth point, lower part of left A-pillar

Earth connection -1-,in front right wiring hamess
Earth connection, in dual tone hom wiring hamess
Connection (75a), in dash panel wiring hamess
Connection, in radiator fan wiring hamess

Connection (87a), in engine wiring hamess

Connection (30, radiator fan), in dash panel wiring hamess
Near ABS control unit
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ioner

% * ® E87 - Control and display unit for air conditioner
X X 4218 - Combi-processor in dash panel insert
3 a 4220 - Motronic control unit
4248 - Diesel direct injection system control unit
J347 - Uttra-sonic sensors control unit
ST - Fuseinfuse carrier
S9 - Fuseinfuse carrier
T2u - 2-pin connector, black, electronics box in footwell, front right
£ T6f - 6-pin connector, black, on dash panel insert
LA o T10d - 10-pin connector, red, connector point, electronics box, plenum chamber
wlwl Ti6a - 16-pin connector, diagnosis connection
7 T26 - 26-pin connector, red, on dash panel insert
L1a T26b - 26-pin connector, yellow, on dash panel insert
Ty Tzengraen grzes  gTem - Earth point, I rt of right A-pil
Tz grac / (=) - Earth point. lower part ofright A-pillar
;1 's @ - Earth connection -1-, in air conditioner wiring hamess.
STAISY, 1% 789 sT2 A (3) - Connecton (speed sgnal), i dash pane wiing harmess
ojh , 9,35 e 72 %a ‘'aa Q @ - Connection (engine speed signal), in dash panel wiring hamess.
w n. -~
o 05 05 @ - Connection (air conditioner compressor), in dash panel wiring harness
Az1 "“ roiws romb! ¥
Az " - - Models with 2.8 1 engine, 142 KW
n:ls n s 035 035 n;ls 42| » = - Models with V8 engine
‘waibl !, gnfli  briro  briro Tisarte Q - Models with diesel engines.
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ioner
€20 - Solarcells

E87 - Control and display unit for air conditioner
G56 - Dash panel temperature sensor

J309 - Solar cellisolation relay

J355 - Solar operation control unit

K - Diagnosis connection

N175 - Heat regulation valve, left
N176 - Heat regulation valve, right

S4 - Fuseinfuse carrier
S7 - Fusein fuse carrier

$25 - Hotair blower single fuse

Tih - Single connector, yellow, electronics box in footwell, front right
Tii - Single connector, yellow, electronics box in footwell, front right
T2u - 2-pin connector, black. electronics box in footwell front right
T3q - 3-pin connector, brown, in plenum chamber, left

Ti6a - 16-pin connector, diagnosis connection

V42 - Temperature sensor blower

VB0 - Coolant circulation pump

m - Positive (+) connection (30a), in dash panel wiring hamess
(;7} - Connection (diagnosis wire K), in dash panel wiring harness
@ - Connection (30, central electrics), in dash panel wiring hamess
@ - Connection, in air conditioner wiring hamess

) - Connection -3-,in air conditioner wiring hamess
%) - Connection (fresh air blower), in auiiary heater wiring hamess

B - Models without solar roof

= - Models with solar roof

Models with petrol engines without auxiiary heater
- Models with diesel engines and models with petrol engines and auxil
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Audi A8 Current Flow Diagram No. 42/4
Intermittent wiper switch
32 b E87 - Control and display unit for air conditioner
X X F129 - Air conditioner pressure switch
G17 - Ambient temperature sensor
G107 - Sunlight penetration photo sensor
G142 - Central vent potentiometer
G238 - Air quality sensor
J31 - Automatic intermittent washfwipe relay
L68 - Dash panel central vent ilumination
Tdi - d-pin connector, black, near central vent, left
Ja1 Ez2 Vs Tdk - 4-pin connector, red, near central vent, right
7 g4 TH0F - 10-pin connector, purple, connector point, wheelhouse, right
Taus £ Tawz l l V5 - Windscreen washer pump
sl e ] (=) - Earth connection -1-,in frontlef wiring harmess
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V1N Overview
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Earth connection -2-, in air conditioner wiring hamess
Connection (C8, air conditioner), in dash panel wiring hamess
Positive (+) connection (53c), in engine compartment wiring hamess
Earth connection, in dash panel wiring hamess

Earth connection (centre console), in dash panel wiring hamess

Models with petrol engines
Models with diesel engines
From 45 KW 1997
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"Air conditioner

D - Ignionistarter switch
2 2 E87 - Control and display unit for air conditioner
X X F73 - Low pressure switch for air conditioner
F183 - Left central vent switch
F184 - Right central vent switch
J44 - Magnetic coupling relay
126 - Blower control unit
J201 - Protective diode
N25 - Airconditioning system magnetic coupling
——1 S5 - Fuseinfuse carrier
Azl o5v a0 S8 - Fusein fuse carier
s Tie - Single connector, green, near compressor
l I I T4 - 4-pin connector, black, near central vent, left
I L ls Tdk - 4-pin connector, red, near central vent, right
S5 S8 iD V2 - Freshai blower
ST3, 75 [Toa N () - Earthpoint, lower part ofright A-pilar
is- 5 () - Positve (+)comnection (15).in dash panel wiing harness
25 25" < b3 @ - Connection (air conditioner -15), in dash panel wiring hamess
i Swiwe swige oS (5) - Comnection -1-in air condioner wiring hamess
i Tain o (%) - Connection -2-, in air conditioner wiring hamess
9.3 o . Q - - Upto 44 kW 1997
I’ ] = - From 45 kW 1997 L
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