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Audi A8 Gurrent Flow Diagram No. 35/8

Digital sound package control unit, Front left treble loudspeaker, Front right treble loudspeaker
J525 - Digital sound package control unit 3

R20 - Frontlefttreble loudspeaker

R22 - Frontrighttreble loudspeaker

TS - 5-pin connector

TEt - 5-pin connector

T17k - 17-pin connector, in right A-pillar coupling station €31
T17m - 17-pin connector, in 7 slot relay carrier 3

T38 - 38-pin connector B3

V344 - Control motor for front let treble speaker

V345 - Control motor for front right treble speaker
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Audi A8 Current Flow Diagram No. 35/9

Digital sound package control unit, Centre eft microphone, Rear left microphone
J525 - Digital sound package control unit 3

J623 - Engine control unit &3

J931 - Power unit mounting control unit

R142 - Centre left microphone

R143 - Centre right microphone

R144 - Rearleft microphone

R145 - Rear right microphone

T2qa - 2-pin connector

T29b - 2-pin connector €3

T29¢ - 2-pin connector B3

T2qd - 2-pin connector

T8ax - 8-pin connector, on right C-pilar

T17h - 17-pin connector, in E-box in engine compartment €3
T32h - 32.pin connector B3

@ - Earth connection 2, in engine compartment wiring hamess

- Earth connection 9, in engine compartment wiring hamess

a1
T } < 2 - According to equipment
T 2 see applicable current flow diagram for engine
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No. 35/10 ~

Audi A8 Current Flow Diagram
Digital sound package control unit, Digital sound package control unit 2

J525 - Digital sound package control unit

J787 - Digital sound package control unit 2 3

T329 - 32-pin connector B3

T32h - 32.pin connector B3
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Eeco
Audi A8 Current Flow Diagram No. 35/ 11
Digital sound package control unit, Digital sound package control unit 2
J525 - Digital sound package control unit
J787 - Digital sound package control unit 2 3
SF2 - Fuse 2in fuse holder F
ST6 - Fuse carrier 6
T329 - 32-pin connector B3
T32h - 32.pin connector B3
T38 - 38.pin connector 3
- - see applicable current flow diagram for fuse assignment
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Current Flow Diagram

igital sound package control u

e —

2, Front left bass loudspeaker, Subwoofer
Digital sound package control unit 2 €3
Frontleft bass loudspeaker

Front right bass loudspeaker
Subwoofer

2-pin connector

2-pin connector

2-pin connector

23-pin connector, on left A-pillar €3
23-pin connector, on right A-pillar 3
27-pin connector, on left A-pillar

27-pin connector, on right A-pillar
32-pin connector B3

Up to May 2011

From June 2011

No. 35/13
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Audi A8 Current Flow Diagram No. 35/13

Digital sound package control unit 2, Rear left bass loudspeaker, Rear right bass loudspeaker
JT87 - Digital sound package control unit 2 €3

R15 - Rearleft bass loudspeaker

RI7 - Rearright bass loudspeaker

T2el - 2-pin connector

T2em - 2-pin connector

T27¢ - 27-pin connector, on right B-pillar €3

T27d - 27-pin connector, on left B-pillar €3

T329 - 32-pin connector B3
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Audi A8 Current Flow Diagram No. 35/2
Radio
R - Radio @
ST6 - Fuse carrier 6 -

SF11 - Fuse 11in fuse holder F

T2de - 2-pin connector B

T10h - 10-pin connector B3

@ - Earth connection 26, in main wiring hamess.

(&) - Earth point 2, on right n luggage compartment &)

. - - see applicable current flow diagram for fuse assignment
STe 2 - Fibre optic cable (FOC)
SFi Bl - =3 - see applicable current flow diagram for data bus network

>

s Lo

100
iy

App <

g

s
o

L H

it

"
b
o
H B
o
W
%

[ 9000150690 | o fan2 [auding [caTA [ || I [l
J o[ 2o
25082023





image2.png
[Current
A service Edt View Settings Warmings 7

=181

&| 8| pl[2[=] 1|« 1] +| o] 2] =[]

R E N E R N — |

Page 2: Radio

e e— [

Audi A8 Current Flow Diagram No. 35/3
Radio, Aerial amplifier
4393 - Convenience system central control unit @31
R - Rado@
RI1 - Aerial
R24 - Acrial amplifier
R47 - Central locking and antitheft alarm system aerial
R93 - Radio aerial 2 -
RI11 - Aerial amplifier 2
RI12 - Aerial amplifier 3
RI70 - Satelite aerial
R183 - Digital radio aerial
R216 - Roof aerial
T2a - 2-pin connector @
T2em - 2-pin connector
T2dd - 2.pin connector 1
T2dg - 2-pin connector
A T2hm - 2-pin connector
] > T4ah - 4-pin connector B
Tdai - 4-pin connector
¥ @ - Earth connection 25, in main wiring hamess.
@ - Earth connection 27, in main wiring hamess.
® a - - Only for American markets
%2 - Only models with no TV receiver
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Audi A8 Current Flow Diagram No. 35/4

Digital sound package control unit, Microphone unit in front roof module
J525 - Digital sound package control unit 3

J533 - Data bus diagnostic interface €3

4794 - Control unit 1 for information electronics &1

R74 - Internal microphone

R140 - Frontleft microphone

ST
srf R141 - Frontright microphone
R164 - Microphone unit in front roof module €31
n SF1 - Fuse 1in fuse holder F ||
ST6 - Fuse carrier 6
T2c0 - 2-pin connector €3
l “ T “ Tek - 6-pin connector B
Prs T8q - 8-pin connector B3
e T32f - 32-pin connector B3
T32h - 32-pin connector B3
s e A 38 - 38.pin connector B
0 VL o ¢ S @ - Earth connection 24, in main wiring hamess.
s
} (72) - Earth point 3, on leftn luggage compartment €31
n o fon Yom ¥ ((oay - Comnection 1 (diagnosis),in main wirng hamess
1 - - see applicable current flow diagram for fuse assignment
@ %2 - see applicable curent flow diagram for preparation for mobile telephone.
"3 - Only models with no TV receiver
@, 4 - Fibre optic cable (FOC)
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Digital sound package control unit, Front left mid-range loudspeaker, Centre loudspeaker
J525 - Digital sound package control unit 3

R103 - Frontleft mid-range loudspeaker

R104 - Front right mid-range loudspeaker

R208 - Centre loudspeaker

R219 - Centre loudspeaker 2

T2es - 2-pin connector

T2t - 2-pin connector

Tdav - 4-pin connector

T17i - 17-pin connector, in coupling point in interior, left &3
T23a - 23-pin connector, on left A-pillar €3

T23b - 23-pin connector, on right A-pillar €3

T27a - 27-pin connector, on left A-pillar

T27b - 27-pin connector, on right A-pillar

T38 - 38-pin connector B3

- From June 2011
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Audi A8 Current Flow Diagram No. 35/6 =
Digital sound package control unit, Left offect loudspeaker, Rear left treble loudspeaker 2
J525 - Digital sound package control unit 3
R209 - Lefteffect loudspeaker
R210 - Right effect loudspeaker
R217 - Rearlefttreble loudspeaker 2
R218 - Rear ight reble loudspeaker 2
Tdaw - 4-pin connector
Tdax - 4-pin connector
T38 - 38-pin connector B3
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Audi A8 Current Flow Diagram No. 35/7

Digital sound package control unit, Rear left treble loudspeaker, Rear left mid-range loudspeaker
J525 - Digital sound package control unit 3
R14 - Rearlefttreble loudspeaker

Ri6 - Rear righttreble loudspeaker

R105 - Rearleft mid-range loudspeaker
R106 - Rear right mid-range loudspeaker
T2da - 2-pin connector

T2dc - 2-pin connector

T2ei - 2-pin connector

T2ek - 2-pin connector

T27¢ - 27-pin connector, on right B-pillar €3
T27d - 27-pin connector, on left B-pillar €3
T38 - 38-pin connector B3
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