	Servicing switches

Removing and installing switches in centre console
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	Removing:

· ‒ → Insert auxiliary tools -C- (making tools => Page 96-3) in holes -D- and pull centre vent evenly out of dash panel insert. 

Note:

Auxiliary tools -C- must not be engaged at centre vent slats, as these could break off.
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	· ‒ → Press respective switch by hand out of holder from rear through dash panel opening. 

· ‒ Then pull out switch as far as it will go and detach connector. 

Installing:

· ‒ Connect connector. 

· ‒ Push switch into recess in dash panel and ensure it is properly located. 

· ‒ Insert centre vent in dash panel opening and ensure it is properly located. 
	


	 

	
	[image: image3.png]




	Making auxiliary tool for removal of dash-panel vents

· ‒ → Bend a 3mm dia. wire into shape illustrated. ø 

· Dimension x = 6 mm. 
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