	Display group 03 at idling speed (engine warm, coolant temperature not below +85 °C)


	
	
	

	
	Read measured value block 3
	→
	▾ Indicated on display
	

	
	800 rpm
	215 mg/H
	211 mg/H
	54 %
	
	

	
	
	
	
	
	Duty cycle (activation) of EGR valve 

 

No specification


	

	
	
	
	
	Intake air mass 

 

If as specified in display zone 2 (tolerance ±20 mg/H (mg/stroke)): okay

 

Intake air mass less than specified: unmetered air in intake tract

Excessive exhaust gas recirculation ⇒ check 

 

Excessive air mass: exhaust gas recirculation less than specified ⇒ check

If engine has been running for 10 min. at idling speed ⇒ Briefly press accelerator 

 

Constant readout: substitute value ⇒ interrogate fault memory


	

	
	
	
	Air mass specified by control unit 

 

180...270 mg/H (mg/stroke): okay

 

Above 270 mg/H (mg/stroke): engine too cold ⇒ run engine till warm

Injection quantity too high ⇒ Readout specifications for injection pump
Intake air temperature very high (display group 7 zone 3) ⇒ adjustment not possible
	

	
	
	Engine speed 

 

740...840 rpm okay


	

	
	
	


