	Display group 04 at idling speed (engine warm, coolant temperature not below +85 °C)


	
	
	

	
	Read measured value block 4
	→
	▾ Indicated on display
	

	
	800 rpm
	2.0° ATDC
	1.6° ATDC
	73 %
	
	

	
	
	
	
	
	Duty cycle (activation) of commencement of injection valve 

 

No specification


	

	
	
	
	
	Current commencement of injection 

 

2° ATDC...3° BTDC: okay

 

Retarded more than 2° ATDC: commencement of injection valve defective

Injection pump retarded much too far
⇒ check injection timing control range, → Chapter 

 

Advanced more than 3° BTDC: engine too cold ⇒ run engine till warm

Injection pump set too advanced
commencement of injection defective
⇒ check injection timing control range, → Chapter
	

	
	
	
	Commencement of injection specified by control unit 

 

2° ATDC...3° BTDC: okay


	

	
	
	Engine speed 

 

740...840 rpm okay


	

	
	
	


