	Testing lambda control

Testing lambda probe signal wire and activation

Note:

The lambda probe signals are monitored by the self-diagnosis system.

· ‒ Interrogate fault memory=>Page 01-7 
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	· ‒ If a lambda probe fault is indicated and probe heater is OK, unplug connector for respective lambda probe at rear of cylinder head. 

· ‒ → Measure voltage between contacts 3 and 4 of connector on wiring harness using hand multimeter V.A.G 1526 (measuring range 2 V). 

· ‒ Switch on ignition. 

· Specified value: 450±50 mV. 

If the specified value is not reached:

· ‒ Connect test box V.A.G 1598/19 to engine control unit wiring harness=>Page 24-15. 

· ‒ Check following wiring connections for open circuit or short circuit to positive or earth: 

Notes:

· ◆ Lambda probe bank 1 -G39 

· ◆ Lambda probe bank 2 -G108 

Engine code ABZ up to 6.96:
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	Connector on wiring harness, contact

Test box V.A.G 1598/19 or engine control unit→ 

3 (-G39)

B20

4 (-G39)

B24

3 (-G108)

B20

4 (-G108)

B23

Engine code ABZ/AKG from 7.96:

Engine code AEW and AHC:

Connector on wiring harness, contact

Test box V.A.G 1598/19 or engine control unit

3 (-G39)

B20

4 (-G39)

B24

3 (-G108)

B21

4 (-G108)

B23

· ‒ If wiring connection is OK, renew engine control unit=>Page 24-16. 
	


