	Windscreen wiper system

Removing and installing windscreen wiper system
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	Note:

Before removing wiper arms, ensure that wiper motor is in park position.

Removing wiper arms:

· ‒ Remove wiper blades. 

· ‒ Lever off cover caps on wiper arms with a screwdriver. 

· ‒ Loosen hexagon nuts (13 mm A/F) -1-, but do not remove completely. 

· ‒ Loosen wiper arms by moving them slightly. 

· ‒ Remove hexagon nuts completely and remove wiper arms. 
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	Removing and installing wiper motor and wiper linkage

· ‒ Removing wiper arms => Page 92-2. 

· ‒ Remove rubber seal from cowl panel trim. 

· ‒ Remove plastic part above left of wiper motor. 

· ‒ Remove three hexagon bolts (10 mm A/F) -1 and 2- and pull cowl panel trim out of the two holders -6-. 

· ‒ Detach hose connection -5- for jets -4- and lift off cowl panel trim. 
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	· ‒ Slacken and remove bolts -2- (6 x 10 mm A/F). 

· ‒ Detach electrical connection at wiper motor. 

· ‒ Remove wiper linkage together with wiper motor from plenum chamber. 

Installing:

Note:

Install wiper linkage in park position shown.

· ‒ Insert wiper linkage together with wiper motor in plenum chamber and make electrical connections. 
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	· ‒ Tighten bolts -2- to 6 Nm. 

· ‒ Connect water hose -5-. 

· ‒ Fit cowl panel trim and screw on with bolts -1 and 2-. 

· ‒ Fit rubber seal at trim. 

· ‒ Move wiper blades to park position => Page 92-6. 
	


