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Tuse, diagnosis connection
Battery

Automatic gearbox control unit

Motronic control unit

Diesel direct injection system control unit

Diagnosis connection

Automatic gearbox control unit fuse

10-pin connector, blue, connector point, electronics box,
plenum chamber

10-pin connector, black, connector point, electronics box,
plenum chamber

10-pin connector, yellow, connector point, electronics box,
plenum chamber

10-pin connector, green, connector point, electronics box,
plenum chamber

16-pin connector, diagnosis connection

26-pin connector, red, on dash panel insert

Selector lever position indicator

- Connection (diagnosis wire K). in dash panel wiring hamess

Positive (+) connection (30), in engine compartment
hamess

ing

- Positive (+) connection (30), in Motronic wiring hamess

Models with 2.8 | engine, 142 kW, engine codes ACK, ALG

Models with 2.5 | TDI-engine, 110 kW, engine codes AFB,
AKN

Models with 3.7 | engine, 170 kW, engine codes AEW, AKJ
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Audi A8 Current Flow Diagram No. 38/3

‘Automatic gearbox control unit,

‘solenoid valves, kick-down switch

F8 - Kick-down switch
¥ b G933 - Gearbox oil temperature sender
;(1 ’!(‘ J104 - ABS with EDL control unit

J217 - Automatic gearbox control unit
N88 - Solenoid valve 1

- Solenoid valve 2

- Solenoid valve 3

- Automatic gearbox pressure control valve -1-

- Automatic gearbox pressure control valve -2-

Automatic gearbox pressure control valve -3-

- Automatic gearbox pressure control valve -4-

- 10-pin connector, black, connector point, electronics box,

plenum chamber

- 10-pin connector, green, connector point, electronics box,

Gz Nss Nos Noo Nzis Nate N1z Nats plenum chamber

16-pin connector, coupling solenoid valve

- Earth point, lower part of right A-

- Earth connection, in dash panel wiring hamess, left
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Earth connection, in dash panel wiring hamess.

- Earth connection (centre console), in dash panel wiring
hamess

Models with front-wheel drive and 2.8 1 or 3.7 | engine.

Ti6h & T166 & 7160 4 T16h 4 T160E T160E TGbA 16 “aw nunr T16n Q>
Im Iu: qu /15 I 1
o8 w0 o o3 s o3 05 o3 n! ns
i B blsw bliws hl!r- biiro mi,. W waisw ].
Iz« |22 s2 !m I;n 22 ln !- Im A

@220

J217

v
@
EN
EN

iw
as
ariws

Jrin

o5
sriws

2
J1oa

aggs=aEggasgy

2

Toroso. 19000000249 W [4D2 [Audi A8 [ACK QY 1




[image: image3.png]g Electronic Service Information System - [Current flowdiagrams] e

& Sevice Edt View Settngs Wamings ?
&| 8| pF|@l®| w0 [1] 2] 0f 2| 2| Blo|g|e|O/s @|=|@|8|2|L| RS .o — &

Page 3 Automatic gearbor control unit fuse, disgnosis connection Search term:
Audi A8 Current Flow Diagram No. 38/4

‘Automatic gearbox control unit, multi-function switch
E20 - Switches and instruments, ighting control

b n E45 - Cruise control system switch
X X F125 - Mult-function switch
G38 - Gearbox speed sender
G182 - Gearbox input speed sender
4217 - Automatic gearbox control unit
4220 - Motronic control unit
119 - Gear selector light bulb
179 - Selector lever ilumination

196 - +- Display illumination (automatic gearbox)

[}
Ex ‘ T2af - connector, yellow, in selector lever console
[ Gas Ga3s G1s2 Gaz TS -

connector, red, in selector lever console
TIGU TISh0  LTi6hg TIGkHO 16615 T16b/6 T160/g T16bi6 Te -

connector, black, on dash panel insert

o8 0,35 n s 0,35 T10a - 10-pin connector, black, connector point, electronics box,
o n e plenum chamber
s — T10g - 10-pin connector, black, near selector lever console
ﬂ::s w Lo A T16b - 16-pin connector, coupling solenoid valve
14 jaz ¥ - Earth connection, in gearbox wiring hamess
o b ¢ > ; o
ol grign g u) - Connection (58d), in dash panel wiring hamess
s J
TogzlTios10 ot a7 v - Earth connection (centre console), in dash panel wiring
I B fez1 hamess
a5 o5 I a @ - Positive (+) connection (15), in cruise control system wiring
o b g g hamess
85 TRargis] B Ko Ko @, * - Models with Tiptronic
05 05 05 05 on  gn om = - Models with CCS
e 3 I—w—l LS N **  _ Red plug connected to black connector ~
[] ] ] we 13 Ja Tz siLe # - Models with 2.8 | engine, 142 kW, engine codes ACK, ALG =
[ # - Models with 2.5 1 TDI-engine, 110 kW, engine codes AFB,
L AKN
### - Models with 3.7 | engine, 170 kW, engine codes AEW, AKJ
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2 3
b . b
X x5 1217 - Automatic gearbox control unit
N110 - Selector lever lock solenoid
6 Fuse in fuse carrier
T2ae - 2-pin connector, black, in selector lever console
T2af - 2-pin connector, yellow, in selector lever console
T8 - 5-pin conneclor, red, in selector lever console
Tsg - 5-pin conneclor, black, in selector lever console
Tée - 6-pin connector, brown, connector point, elecironics box,
plenum chamber
T10 - 10-pin connecor, blue, connector point, electronics box,
plenum chamber
T10a - 10-pin connector, black, connector point, electronics box,
) plenum chamber
Uz = T10b - 10-pin connecor, yellow, connector point, electronics box,
A plenum chamber
05" 05 05" 05 T10c - 10-pin connecor, green, connector point, electronics box,
aige e awige swige < plenum chamber
s Nss !,, Jzur - T10g - 10-pin connector, black, near selector lever console
Earth connection, in gearbox wiring hamess
5 ‘ 8 sT3 (02
£ : : 104/ () - Earth connection, selector lever ilumination
O I“ I" |“ IZ 3 2N (i2) - Posiive (+) connection (16), in dash panel wing harness
o5 o5 as o5 0 @ 7o) - Earth connection, in dash panel wiring harness
brko et 9”;" rolas swioe Y @ Connection -1- (15), in automatic gearbox wiring hamess.
T T \z'r‘mimnminms s 5 Models vith Tiptor
45 @5 o5 65 o3 a8 os 1o 0 - Models with 2.8 | engine, 142 kW, engine codes ACK and ALG
bows  we o brow geil peian raige swige swige and 25 | TDI-engine, engine codes AFB and AKN
ETM;E-E,M:-EM hw,hwq:m‘;i‘ :'ﬁwi'ﬁw{ - Wodels wih 37 engine, 70 KW, engine codes AEW and
15 95 05 05 05 05 03 o5 os 07
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‘Brake TighT SWitch, Starter INIBITor Telay, Teversing Tig &
3 b 3 B - Starter
x X D - Ignition/starter switch
3 B E1 - Lighting switch
Y tamson F - Brake light switch
- 4123 - Bulb monitoring device
B 3207 J207 - Starter inhibitor rela
y
10 oo 1emt 20 4220 - Motronic control unit
4267 - Mirror memory control unit
30 S0 sus0Rsas0Rsan Feam M - it bul, left
Mo - . right
13 M6 - light bulb, left
10 25 25 05 05 M7 - ight bulb, right
bira swira swiro mwiro guiwr S3 - Fusein fuse carier
o I I [ 3 ST - Fusein fuse carrier
B D $9 - Fusein fuse carrier
LY e 0 [ IS, B, N Teb - 5;;:;; comnector, grey, foatwel igh,atwheslhouse, behind
) e biiro n on @
7 W, ’l T 3 ¢ > T10 - 10-pin connector, blue, connector point, electronics box,
A A e I plenum chamber
ST1 (3] 9,89 ! g2 220 Ry T10d - 10-pin connector, red, connector point, electronics box,
’. 13 “‘ﬂu 152 obie Foart Tion v plenum chamber
7a '9a g9a T14 - 14-pin connector, purple, behind steering column switch trim
15 10 05 b [} - Earth connection, in tailgate/bootid wiring hamness
blra  blro b - Connection (54), in dash panel wiring hamess.
I, T ¥ S
Joor ECI
S§T2 a - Connection (mutti-function switch), in dash panel wiring
- haess

Connection -1-, in tailgate/bootiid wiring hamess

Models with 2.8 | engine, 142 kW, engine codes ACK, ALG
Models with 2.5 | TDI-engine, 110 kW, engine codes AFB,
AKN

Models with 3.7 | engine, 170 kW, engine codes AEW, AKJ

(=)
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@ - Connection (58a), in dash panel wiring hamess
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