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Relay for glow plugs, glow plugs

952 - Glow plug relay
J495 - Glow plug relay 2 €31
Q10 - Glow plug-1-
Q11 - Glow plug 2-
Q12 - Glow plug 3-
Q13 - Glow plug 4-
Q14 - Glow plug -5-

Q15 - Glow plug -6-

L Q16 - Glow plug 7-

w© Q17 - Glow plug 8-

- $39 - Fuse 1 for glow plugs - engine £

$125 - Fuse 2 for glow plugs - engine

- Connection (glow plugs), in front right wiring hamess

- Connection (glow plugs), in engine compartment wiring
hamness
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sel direct inje
supply relay
4248 - Diesel direct injection system control unit

J317 - Terminal 30 voltage supply relay B3

n system control unit, terminal 30 voltage

J518 - Entry and start authorisation control unit €3
Ti7a - 17-pin connector, black, in electronics box, plenum chamber
TI7d - 17-pin connector, blue, in electronics box, plenum chamber
Jm @
A7 (32 - Earth point, lower part of right A pillar 31
Do’s nﬁs b’:s @ - Earth connection -1-, in engine compartment wiring hamess
vio  blow sur
") - Earth connection -2-, in engine compartment wiring harness
~ Positive (+ . .
T bt T g i) - Positve (+) connection -2- (87), in interior wiring harness
= 2, @ - Positive (+) connection (30). in main wiring hamess
T @ - Positive (+) connection -4- (30), in main wiring hamess
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iesel direct injection system control unit, fuel pressure regulating
valve, water spray protection flap valve in intake manifold, fuel
metering valve
J248 - Diesel direct injection system control unit

’ N276 - Fuel pressure regulating valve

N290 - Fuel metering valve
N397 - Water spray protection flap valve in intake manifold

SC21 - Fuse -21- on fuse box €
SC28 - Fuse -26- on fuse box €

rrx Ti7b - 17-pin connector, green, in electronics box, plenum chamber
rolar oigr  roigr  rolar
l l T17c - 17-pin connector, brown, in electronics box, plenum chamber
iz
Torans B Ti7e - 17-pin connector, red, in electronics box. plenum chamber
7o @ - Positive (+) connection -1- (15), in engine compartment wiring
hamess
1.3 LA S S X IS o) - Connection -3-, in engine compartment wiring hamess
iy o g oo b - Connection (87a), in diesel direct injection system wiring
@ hamess
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sel direct injection system control unit, coolant temperature
sender, oil temperature sender, fuel temperature sender, air mass
meter, engine speed sender, Hall sender, fuel pressure sender, oil
pressure switch

F1 - Oil pressure switch
G8 - Oiltemperature sender
G28 - Engine speed sender
G40 - Hallsender
G62 - Coolant temperature sender
G70 - Airmass meter
GB1 - Fuel temperature sender
G247 - Fuel pressure sender
G G 1248 - Diesel direct injection system control unit
® ® © T3c - 3-pin connector, grey, on engine speed sender
Tém - 6-pin connector, black, i compartment, left
I"" "’s I”‘“ v r“ I” TI7b - |E7£>mcnnneaon green, in electronics box, plenum chamber
o am o o5 o5 o5 A @ - Earth connection engine compartment wiring harness

| Q b @ - Earth connection engine compartment wiring harness

- Earth connection -4-, in engine compartment wiring hamess
L L, o (=) ine com o
' - Earth connection (screening), in engine compartment wiring
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Diesel direct injection system control unit, brake light switch

ca
F
Fa7

J104
J217
J248
J393
J518

PODEY § FgLe

oo}

Suppression fiter
Brake light switch

Cruise control system brake pedal switch (diesel direct injection

system)
ABS with EDL control unit @1

Automatic gearbox control unit €3

Diesel direct injaction system control unit
Convenience system central control unit @31
Entry and start authorisation control unit 3
Fuse -12- on fuse box €

Fuse -22- on fuse box €

Fuse -38- on fuse box €

17-pin connector, brown, in electronics box, plenum chamber

17-pin connector, blue, in electronics box, plenum chamber

o]

Earth connection -12-,

in main wiring harness
Connection -1- (54), in main wiring haress
Connection -2- (54), in main wiring haress
Connection -5-, ing hamess

m
Connection 7.

engine compartment wiring harness
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Diesel direct injection system control unit, injectors for cylinders 1,
4,6and 7, fuses
J248 - Diesel direct injection system control unit

N30 - Injector. cylinder 1
N33 - Injector. cylinder 4
' N84 - Injector. cylinder 6
N85 - Injector. cylinder 7

SC5 - Fuse -5- on fuse box €
SC6 - Fuse -6- on fuse box £
SC7 - Fuse -7- on fuse box €
SC19 - Fuse -19- on fuse box €
SC29 - Fuse -29- on fuse box €

SC31 - Fuse -31- on fuse box €
Ti7a - 17-pin connector, black, in electronics box, plenum chamber

@ - Positive (+) connection -3- (87), in interior wiring harness

Connection -1-, in diesel direct injection system wiring harness
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Diesel direct injection system control unit, throttle valve modul
turbocharger 1 control ut

Ed5
J217
4248
1338
Js27
J724

- Connection (high bus), i

, intake manifold flap motor
Cruise control system switch

Automatic gearbox control unit €3

Diesel direct injaction system control unit
Throttle valve module

Steering column electronics control unit @31
Turbocharger 1 control uni
46-pin connector, black, diagnosis connection

46-pin connector, on steering column electronics control unit
47-pin connector, black, in electronics box, plenum chamber
o]

17-pin connector, brown, in electronics box, plenum chamber
o]

17-pin connector, black, connector A, relay carrier, footwell,
driver's side

46-pin connector, black, CAN bus separating connector, ight
Intake manifold flap motor

Earth connection -1-, in engine compartment wiing harness

compartment wiring harness

Connection (low bus), in engine compartment wiring hamess

Connection (K diagnosis wiing). in engine compartment wiring
hamess
Connection -1-,

CAN bus (data

diesel direct injection system wiring hamess

re)
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valve, kick-down switch, accelerator pedal position senders,
electrolhydraulic engine mounting solenoid valve, torque rod valve,
charge air pressure sender, intake air temperatur

F8 - Kick-down switch

G31 - Charge air pressure sender
G42 - Intake air temperature sender
G79 - Accelerator pedal position sender
G185 - Accelerator pedal position sender -2-
I e e | 4248 - Diesel direct injection system control unit
s N18 - Exhaust gas recirculation valve
ol N145 - Electro/ydraulic engine mounting solenoid valve, right
N382 - Torque rod valve
Ti7e - 17-pin connector, brown, in electronics box, plenum chamber
Nis Nez
TI7d - 17-pin connector, blue, in electronics box, plenum chamber

o]

x 05 A @ - Earth connection -7-, in main wiring hamess
o ..
] > @ - Connection -1-, in diesel direct injection system wiring hamess
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iesel direct injection system control unit, radiator fan, exhaust gas
temperature sender -

Exhaust gas temperature sender -1-
Diesel direct injaction system control unit

Fuse -8- on fuse box €

Fuse -17- on fuse box €

17-pin connector, black, in electronics box, plenum chamber

47-pin connector, red, in electronics box, plenum chamber
Radiator fan

Radiator fan -2-

Earth point, lower part of right A pillar €3

Positive (+) connection -1- (87a), in main wiring hamess

Connection -2-,in diesel direct injection system wiring harness
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Diesel direct injection System control unit 2, injectors 2, 3, 5 and 6,
exhaust gas recirculation valve -2-, left electrolhydraulic engine
‘mounting solenoid valve, intake manifold flap 2 motor

J434 - Diesel direct injection system control unit 2

N31 - Injector. cylinder 2
' N32 - Injector, cylinder 3
N83 - Injector. cylinder 5
N86 - Injector. cylinder &
N144 - Electro/hydraulic engine mounting solenoid valve, left
s s N213 - Exhaust gas recirculation valve

V275 - Intake manifold flap 2 motor
@ - Earth connection -2-, in engine compartment wiring harness

(722) - Connection -2-in diesel diect injection system wiring hamess

>

e bibe

' l < 9
e Jisi Mo v
® '
'w r.s Im 'A. F, a
o B oss LN
a5 g S

a

7

Nl Nz Nes| N

aggs=aEggasgy

W 1s 67 e 1% 160 1ol ez 63 iee 165 186 167 _ts8





image17.png
sel direct injection system control unit 2, throttle valve module 2,
turbocharger 2 control unit
4494 - Diesel direct injection system control unit 2
J544 - Throtlle valve module 2

’ J725 - Turbocharger 2 control uni

@ - Earth connection engine compartment wiring harness
(i37) - Earth connection

(72) - Connection 2

. - CAN bus (data wire)

engine compartment wiring harness

diesel direct injection system wiring hamess
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n system control unit 2, air mass meter 2,

exhaust gas temperature sender -1-, bank 2

G236
G246
1494
Ti7b

(=)

131

Exhaust gas temperature sender -1-, bank 2
Air mass meter 2
Diesel direct injection system control unit 2

17-pin connector, green. in electronics box, plenum chamber

Earth connection
Earth connection

engine compartment wiring harness

engine compartment wiring harness
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Fuel cooling pump relay, high pressure sender, fuel cooling pump,
heater element (crankcase breather), coolant shut.off valve
G65 - High pressure sender

3217 - Automatic gearbox control unit €31

4255 - Climatronic control unit
J445 - Fuel cooling pump relay €31
N79 - Heater element (crankcase breather)

N82 - Coolant shut-off valve

SC3 - Fuse 3 on fuse box €
SC16 - Fuse 16 on fuse box
8C22 - Fuse 22 on fuse box

2 Ti7a - 17-pin connector, black, in electronics box, plenum chamber
fnse=
= Ti7b - 17-pin connector, green, in electronics box, plenum chamber
Ti7e - 17-pin connector, red, in electronics box, plenum chamber
o e o8 o3 A V166 - Fuel cooling pump
Q Y @ - Earth connection 1, in engine compartment wiring hamess
73 - Earth connection 4, in engine compartment wiring hamess
o _ywira Reier e N -
@ - Earth connection 10, in main wiring hamess.
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Control unit with display in dash panel insert, fuel pump relay

G
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G237
Nt

J285
SF10
Tda
Tee
T32
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- Fuel gauge sender
- Fuel pump (pre-supply pump)

- Fuel gauge sender 3

- Fuel pump relay

- Control unit with display in dash panel insert 3

- Fuse 10 on fuse box @

- 4-pin connector, under cover, right, on vehicle floor
connector, under cover, right, on vehicle floor

- 32-pin connector, bue, on dash panel insert

- Earth connection (fuel gauge sender), in main wiring harness

- Earth connection 25, in main wiring hamess
- Earth point 2, in luggage compartment, right €31

- Positive (+) connection 1 (87), in interior wiring hamess
- Positive (+) connection 3 (30), in main wiring hamess
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Control unit with
fuel gauge senders,

lay in dash panel insert, fuel gauge, fuel pump,
pressure warning lamp

F66 - Coolant shortage indicator switch
Gl - Fuelgauge
G23 - Fuel pump

{ G169 - Fuel gauge sender 2
G266 - Oil level thermo sender

G393 - Fuel gauge sender 4
J285 - Control unit with display in dash panel insert €31
T 1 K3 - Ol pressure waming lamp

w0 oS

i N K28 - Coolant temperature/coolant shortage warning lamp
A i SB10 - Fuse 10 on fuse box
SBn SF9 - Fuse 9 on fuse box
S Tda - 4-pin connector, under cover, right, on vehicle floor
os Tée - 6-pin connector, under cover, right, on vehicle floor
Ti7a - 17-pin connector, black, in electronics box, plenum chamber
A
TI7d - 17-pin connector, blue, in electronics box, plenum chamber
€ 2 o]
T32 - 32-pin connector, blue, on dash panel insert

- Earth connection 2, in engine compartment wiring hamess
@G ® Jass &K FKa (

- Earth connection (fuel gauge sender), in main wiring harness

()
(=)
@ - Earth connection (sender earth), in interior wiring harness.
@
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T | T T T Tz - Earth point 2, in luggage compartment, right €31
& ' - Positive (+) connection 1 (15a), in main wiring harness
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Edition 02.2004

Audi A8 4.0 litre turbo-diesel engine (202 kW - 8-cylinder), engine code ASE
From model year 2003

Fuse box, dash panel, left

Fuse colours
30A- green
25A- white
20A- yellow
15 A~ blue
10A- red
75 A~ brown
5A- beige
1A- black
SB - Fuses in fuse box, dash panel, left
SC - Fuses in fuse box, dash panel, right
SD - Fuses in fuse box, luggage compartment, left
SF - Fuses in fuse box, luggage compartment, right

Fuse box, dash panel, right
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Relay carrier, electronics box, plenum chamber

Position of relays
1- Relay for glow plugs (J52)
2- Relay 2 for glow plugs (J495)
3 - Terminal 30 voltage supply relay (J317)
B~ Fuse 1 for glow plugs - engine (S39)
C - Fuse 2 for glow plugs - engine (S125)

Relay and fuse carrier, behind dash panel, left

Position of relays
3 - Terminal 15 voltage supply relay (J329)
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Relay carrier, front passenger's footwell

Position of relays
1.1 - Fuel cooling pump relay (J445)
2- Starter motor relay (J53)
3 - Starter motor relay -2- (J695)

Position of components in: main fuse carrier, A

r, right

T

1A~ Screw connection for radiator fan 1
2- Radiator fan fuse, 2nd speed (S104, 60 A)
2A - Screw connection for radiator fan 2
3~ Screw connection for terminal 30 (battery)
4~ Screw connection for terminal 30 (starter)
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Relay and fuse carrier, luggage compartment, right
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Position of relays
3~ Fuel pump relay (J17)
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Page 2 Battery, energy management control unit, battery cut-off relay
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Battery, energy management control unit, battery cut-off relay
A - Battery

J234 - Airbag control unit B3

J644 - Energy management control unit &3

655 - Battery cut-offrelay

131 - Fuse 1, 110 A, in luggage compartment, rear right €3

- Fuse 2, 60 A in luggage compartment, rear right

- Fuse 3, 150 A, in luggage compartment, rear right €31

- Fuse -15- on fuse box @3

- Fuse -36- on fuse box @31

- 46-pin connector, black, CAN separating connector, right
- Heated windscreen

- Earth strap, engine - body

Earth point, on cylinder block

- Earth connection -14-, in main wiring harness
- Positive (+) connection -7- (30), in main wiring hamess

CAN bus (data wire)
In luggage compartment, rear right

QDR TEEE
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Starter, alternator, terminal 15 voltage supply relay, starter motor

relay
B - Starer
C - Attemator
C1 - Voltage regulator
' J53 - Starter motor relay €3
J329 - Terminal 15 voltage supply relay B3
J518 - Entry and start authorisation control unit &3
T — J695 - Starter motor relay -2- €1
o5 Lo s 42 - Radiator fan single fuse €3
104 - Radiator fan fuse, 2nd speed @31
2 SC3 - Fuse -9- on fuse box
g g% - 2-pin connector, black, in engine compartment, front right
o - 2-pin connector, black, on alterator

T2a
T2
TV1 - Junction box
@ - Positive (+) connection -2- (15), in interior wiring hamness
@ - Positive (+) connection (15), in main wiring hamess

4 l € ¥ (e - Posiive (+) connecton (50, in main wirng haress
@ - Positive (+) connection -2- (30), in main wiring hamess
@ - Positive (+) connection -6- (30), in main wiring hamess

Main fuse carier, A pilla. right
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