Âåðñèÿ VAG-COM: Âåðñèÿ 311.2-N

Íîìåð Êîíòðîëëåðà: 4D0 907 558 N  

  Êîìïîíåíò è/èëè Âåðñèÿ: 3.7L V8/5V          0003

           Ïðîãðàììíûé Êîä: 11753

           Êîä Àâòîöåíòðà: WSC 85555

Äîïîëíèòåëüíàÿ èíôîðìàöèÿ: WAUZZZ4DZ1N010044     AUZ7Z0Y1644973

15 Ïîèñê Íåèñïðàâíîñòåé:

17985 - Right Engine Mount Solenoid Valve (N145): Open Circuit

        P1577 - 35-10 - - - Íåóñòîé÷èâ

16814 - Catalyst System: Bank 2: Efficiency Below Threshold

        P0430 - 35-10 - - - Íåóñòîé÷èâ

17652 - Fuel Injector for Cylinder 8 (N86): Open Circuit

        P1244 - 35-10 - - - Íåóñòîé÷èâ

17645 - Fuel Injector for Cylinder 1 (N30): Open Circuit

        P1237 - 35-10 - - - Íåóñòîé÷èâ

17648 - Fuel Injector for Cylinder 4 (N33): Open Circuit

        P1240 - 35-10 - - - Íåóñòîé÷èâ

17649 - Fuel Injector for Cylinder 5 (N83): Open Circuit

        P1241 - 35-10 - - - Íåóñòîé÷èâ

17647 - Fuel Injector for Cylinder 3 (N32): Open Circuit

        P1239 - 35-10 - - - Íåóñòîé÷èâ

17650 - Fuel Injector for Cylinder 6 (N84): Open Circuit

        P1242 - 35-10 - - - Íåóñòîé÷èâ

17646 - Fuel Injector for Cylinder 2 (N31): Open Circuit

        P1238 - 35-10 - - - Íåóñòîé÷èâ

17651 - Fuel Injector for Cylinder 7 (N85): Open Circuit

        P1243 - 35-10 - - - Íåóñòîé÷èâ

17978 - Engine Start Blocked by Immobilizer

        P1570 - 35-10 - - - Íåóñòîé÷èâ

16684 - Random/Multiple Cylinder Misfire Detected

        P0300 - 35-10 - - - Íåóñòîé÷èâ

16685 - Cylinder 1 Misfire Detected

        P0301 - 35-10 - - - Íåóñòîé÷èâ

16804 - Catalyst System: Bank 1: Efficiency Below Threshold

        P0420 - 35-10 - - - Íåóñòîé÷èâ

16689 - Cylinder 5 Misfire Detected

        P0305 - 35-10 - - - Íåóñòîé÷èâ

