	With spring clip for mounting brake light switch.
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	· 1 - Brake pedal stop surface 

· 2 - Spring clip 

· 3 - Pedal bracket 

· 4 - Brake light switch -F- 

· a - Dimension: max. 1.2 mm - min. 0.5 mm 

Note:

· The switch must only be fitted once to ensure that it is sufficiently tight.

· ‒ Press spring clip -2- into the pedal bracket, against the direction of travel. 

· ‒ Guide switch -4- into the installed spring clip -2- and press or screw it up to stop. 

· This must not place the brake pedal under any pre-tension.

· ‒ Check dimension -a- with feeler gauge and, if necessary, turn brake light switch to dimension -a-. 
	


