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	Always read rules for cleanliness and instructions for working on fuel system → Chapter.



	Follow these instructions before starting work and while working on the fuel system.






	
	


[image: C:\ElsaWin\graphics\wi\A23-0202.png]
	1 - 
	Fuel metering valve -N290-



	2 - 
	High-pressure pump



	3 - 
	Fuel pressure sender -G247-



	4 - 
	Distributor housing with high-pressure control circuit



	5 - 
	Fuel pressure regulating valve -N276-



	6 - 
	Rail element (high-pressure accumulator)



	 
	For cylinder bank 1



	7 - 
	Rail element (high-pressure accumulator)



	 
	For cylinder bank 2



	8 - 
	Injectors



	 
	5 ... 8



	 
	Cylinder bank 2



	9 - 
	Injectors



	 
	1 ... 4



	 
	Cylinder bank 1



	10 - 
	Mechanical crash valve



	11 - 
	Baffle housing



	12 - 
	Fuel pre-supply pump -G6-



	 
	Pre-supply pump



	13 - 
	Fuel bypass valve -N312-



	14 - 
	Fuel pump -G23-



	15 - 
	Fuel cooler (air)



	 
	On underside of vehicle



	16 - 
	Bimetallic preheating valve



	17 - 
	Fuel cooler



	 
	Water low-temperature circuit



	18 - 
	Fuel filter



	19 - 
	Gear pump
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